(footprint "NetTie-3_THT_Pad0.3mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Net tie, 3 pin, 0.3mm round THT pads")
	(tags "net tie")
	(property "Reference" "REF**"
		(at 1.2 -1.3 0)
		(layer "F.SilkS")
		(hide yes)
	)
	(property "Value" "NetTie-3_THT_Pad0.3mm"
		(at 1.2 1.3 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr exclude_from_pos_files exclude_from_bom allow_missing_courtyard)
	(net_tie_pad_groups "1, 2, 3")
	(pad "1" thru_hole circle
		(at 0 0)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 1.2 0)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 2.4 0)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
)
