(footprint "Finder_34.81"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Relay SPST, Finder Type 34.81 (opto relays/coupler), vertical/standing form, see https://gfinder.findernet.com/public/attachments/34/EN/S34USAEN.pdf")
	(tags "Relay SPST Finder")
	(property "Reference" "REF**"
		(at 10.25 -2.2 0)
		(layer "F.SilkS")
	)
	(property "Value" "Finder_34.81"
		(at 9.15 4.8 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 10.25 2.4 0)
		(layer "F.Fab")
	)
	(pad "11" thru_hole circle
		(at 16.25 0)
		(size 2.4 2.4)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole circle
		(at 21.25 0)
		(size 2.4 2.4)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A1" thru_hole roundrect
		(at 0 0)
		(size 2.4 2.4)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.104)
	)
	(pad "A2" thru_hole circle
		(at -3.75 0)
		(size 2.4 2.4)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/OptoDevice.3dshapes/Finder_34.81.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
