(footprint "Lightpipe_Bivar_RLP1-400-650"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "1-way, 2.8mm lightpipe, 10mm lens output height, 17mm protrusion, https://www.bivar.com/parts_content/Datasheets/RLP1-XXX-XXX.pdf")
	(tags "planar light pipe 1 way 3mm ")
	(property "Reference" "REF**"
		(at -5.6 3.05 0)
		(layer "F.SilkS")
	)
	(property "Value" "Lightpipe_Bivar_RLP1-400-650"
		(at 0 -1.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(fp_text user "${REFERENCE}"
		(at -1.75 0 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole oval
		(at 0 -4.15)
		(size 2.5 2)
		(drill oval 2.5 2)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole oval
		(at 0 4.15)
		(size 2.5 2)
		(drill oval 2.5 2)
		(layers "F&B.Cu" "*.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/OptoDevice.3dshapes/Lightpipe_Bivar_RLP1-400-650.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
