(footprint "Lightpipe_LPF-C013301S"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "https://www.lumex.com/spec/LPF-C013301S.pdf")
	(tags "lightpipe triple tower right angle 3mm")
	(property "Reference" "REF**"
		(at -4.5 9.3 270)
		(layer "F.SilkS")
	)
	(property "Value" "Lightpipe_LPF-C013301S"
		(at 2.6 8.2 270)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr exclude_from_pos_files)
	(fp_text user "${REFERENCE}"
		(at -2.5 9.3 90)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -2.6 0.7 180)
		(size 1.25 1.25)
		(drill 1.25)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 2.6 17.1 180)
		(size 1.25 1.25)
		(drill 1.25)
		(layers "*.Cu" "*.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/OptoDevice.3dshapes/Lightpipe_LPF-C013301S.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
