(footprint "Osram_BPW34S-SMD"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "PhotoDiode, plastic SMD DIL, 4.5x4mm, area: 2.65x2.65mm, https://dammedia.osram.info/media/resource/hires/osram-dam-5488319/BPW%2034%20S_EN.pdf")
	(tags "PhotoDiode plastic SMD DIL")
	(property "Reference" "REF**"
		(at 0.01 -3.2 0)
		(layer "F.SilkS")
	)
	(property "Value" "Osram_BPW34S-SMD"
		(at 0 3.17 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0.01 -3.2 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -3.05 0 180)
		(size 1.3 1.9)
		(layers "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "" smd roundrect
		(at -3.05 0 180)
		(size 1.5 2.1)
		(layers "F.Mask")
		(roundrect_rratio 0.125)
	)
	(pad "" smd roundrect
		(at 3.05 0 180)
		(size 1.3 1.1)
		(layers "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "" smd roundrect
		(at 3.05 0 180)
		(size 1.5 1.3)
		(layers "F.Mask")
		(roundrect_rratio 0.125)
	)
	(pad "1" smd roundrect
		(at -3.05 0 180)
		(size 1.4 2)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.125)
	)
	(pad "2" smd roundrect
		(at 3.05 0 180)
		(size 1.4 1.2)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.125)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/OptoDevice.3dshapes/Osram_BPW34S-SMD.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
