(footprint "Oscillator_OCXO_Morion_MV317"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "https://www.morion-us.com/catalog_pdf/mv317.pdf")
	(tags "OCXO")
	(property "Reference" "REF**"
		(at 0 -5 0)
		(layer "F.SilkS")
	)
	(property "Value" "Oscillator_OCXO_Morion_MV317"
		(at 9.5 12.2 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "Uref"
		(at -2 0 270)
		(layer "F.SilkS")
	)
	(fp_text user "RF"
		(at 21 19 270)
		(layer "F.SilkS")
	)
	(fp_text user "Us"
		(at -2 19 270)
		(layer "F.SilkS")
	)
	(fp_text user "Uin"
		(at 21 0 270)
		(layer "F.SilkS")
	)
	(fp_text user "GND"
		(at 21 9.5 270)
		(layer "F.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at 10.05 10.35 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 0 19.05 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 19.05 19.05 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 19.05 9.525 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 19.05 0 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Oscillator.3dshapes/Oscillator_OCXO_Morion_MV317.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
