(footprint "Texas_DSBGA-6_0.757x1.01mm_Layout2x3_P0.35mm"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Texas Instruments, DSBGA-6, 0.757x1.01mm, SMD, YKA0006 pad definition, 0.757x1.01mm, 6 Ball, 2x3 Layout, 0.35mm Pitch, https://www.ti.com/lit/ds/symlink/tps62843.pdf")
	(tags "BGA 6 0.35 TI 0.787x1.04mm (max)")
	(solder_mask_margin -0.0325)
	(solder_paste_margin -0.0275)
	(property "Reference" "REF**"
		(at 0 -1.505 0)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_DSBGA-6_0.757x1.01mm_Layout2x3_P0.35mm"
		(at 0 1.505 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 -90)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -0.175 -0.35)
		(size 0.21 0.21)
		(layers "F.Paste")
		(roundrect_rratio 0.184524)
	)
	(pad "" smd roundrect
		(at -0.175 0)
		(size 0.21 0.21)
		(layers "F.Paste")
		(roundrect_rratio 0.184524)
	)
	(pad "" smd roundrect
		(at -0.175 0.35)
		(size 0.21 0.21)
		(layers "F.Paste")
		(roundrect_rratio 0.184524)
	)
	(pad "" smd roundrect
		(at 0.175 -0.35)
		(size 0.21 0.21)
		(layers "F.Paste")
		(roundrect_rratio 0.184524)
	)
	(pad "" smd roundrect
		(at 0.175 0)
		(size 0.21 0.21)
		(layers "F.Paste")
		(roundrect_rratio 0.184524)
	)
	(pad "" smd roundrect
		(at 0.175 0.35)
		(size 0.21 0.21)
		(layers "F.Paste")
		(roundrect_rratio 0.184524)
	)
	(pad "A1" smd circle
		(at -0.175 -0.35)
		(size 0.265 0.265)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask")
	)
	(pad "A2" smd circle
		(at 0.175 -0.35)
		(size 0.265 0.265)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B1" smd circle
		(at -0.175 0)
		(size 0.265 0.265)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B2" smd circle
		(at 0.175 0)
		(size 0.265 0.265)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask")
	)
	(pad "C1" smd circle
		(at -0.175 0.35)
		(size 0.265 0.265)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask")
	)
	(pad "C2" smd circle
		(at 0.175 0.35)
		(size 0.265 0.265)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask")
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_BGA.3dshapes/Texas_DSBGA-6_0.757x1.01mm_Layout2x3_P0.35mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
