(footprint "DFN-6_1.3x1.2mm_P0.4mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "6-Lead Plastic DFN (1.3mm x 1.2mm) ")
	(tags "DFN 0.4")
	(property "Reference" "REF**"
		(at 0 -1.7 0)
		(layer "F.SilkS")
	)
	(property "Value" "DFN-6_1.3x1.2mm_P0.4mm"
		(at 0 1.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0.025 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -0.368 -0.4)
		(size 0.53 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -0.368 0)
		(size 0.53 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -0.368 0.4)
		(size 0.53 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 0.368 0.4)
		(size 0.53 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 0.368 0)
		(size 0.53 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 0.368 -0.4)
		(size 0.53 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/DFN-6_1.3x1.2mm_P0.4mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
