(footprint "Infineon_PG-TSNP-6-10_0.7x1.1mm_0.7x1.1mm_P0.4mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "6 lead, 1.1x0.7mm body, 0.37mm height, TSNP (https://www.infineon.com/cms/en/product/packages/PG-TSNP/PG-TSNP-6-10/)")
	(tags "PG-TSNP-6-10 TSNP")
	(property "Reference" "REF**"
		(at 0 -1.6 0)
		(layer "F.SilkS")
	)
	(property "Value" "Infineon_PG-TSNP-6-10_0.7x1.1mm_0.7x1.1mm_P0.4mm"
		(at 0 1.2 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0.77 0 90)
		(layer "F.Fab")
	)
	(pad "" smd circle
		(at -0.2 -0.4)
		(size 0.25 0.25)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at -0.2 0)
		(size 0.25 0.25)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at -0.2 0.4)
		(size 0.25 0.25)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 0.2 -0.4)
		(size 0.25 0.25)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 0.2 0)
		(size 0.25 0.25)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 0.2 0.4)
		(size 0.25 0.25)
		(layers "F.Paste")
	)
	(pad "1" smd roundrect
		(at -0.2 -0.4)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "2" smd roundrect
		(at -0.2 0)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "3" smd roundrect
		(at -0.2 0.4)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "4" smd roundrect
		(at 0.2 0.4)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "5" smd roundrect
		(at 0.2 0)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "6" smd roundrect
		(at 0.2 -0.4)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_LGA.3dshapes/Infineon_PG-TSNP-6-10_0.7x1.1mm_0.7x1.1mm_P0.4mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
