(footprint "Rohm_MLGA010V020A_LGA-10_2x2mm_P0.45mm_LayoutBorder2x3y"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Rohm  LGA, 10 Pin (https://fscdn.rohm.com/en/techdata_basic/ic/package/Jisso_MLGA010V020A-1-2_Rev005s_E2(MSL3).pdf)")
	(tags "Rohm LGA NoLead")
	(property "Reference" "REF**"
		(at 0 -2.15 0)
		(layer "F.SilkS")
	)
	(property "Value" "Rohm_MLGA010V020A_LGA-10_2x2mm_P0.45mm_LayoutBorder2x3y"
		(at 0 1.8 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 90)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 90)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.865 -0.45 90)
		(size 0.25 0.58)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -0.865 0 90)
		(size 0.25 0.58)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -0.865 0.45 90)
		(size 0.25 0.58)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -0.23 0.865 90)
		(size 0.58 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at 0.22 0.865 90)
		(size 0.58 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at 0.865 0.45 90)
		(size 0.25 0.58)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at 0.865 0 90)
		(size 0.25 0.58)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at 0.865 -0.45 90)
		(size 0.25 0.58)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at 0.22 -0.865 90)
		(size 0.58 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at -0.23 -0.865 90)
		(size 0.58 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_LGA.3dshapes/Rohm_MLGA010V020A_LGA-10_2x2mm_P0.45mm_LayoutBorder_3x2y.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
