(footprint "SIP3_11.6x8.5mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "RECOM,R78EXX,https://www.recom-power.com/pdf/Innoline/R-78Exx-0.5.pdf")
	(tags "SIP3 Regulator Module")
	(property "Reference" "REF**"
		(at 2.54 3.3 180)
		(layer "F.SilkS")
	)
	(property "Value" "SIP3_11.6x8.5mm"
		(at 2.54 -8 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 2.54 -2.7 180)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0 270)
		(size 1.3 1.3)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 2.54 0 180)
		(size 1.3 1.3)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 5.08 0 270)
		(size 1.3 1.3)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SIP.3dshapes/SIP3_11.6x8.5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
