(footprint "PowerIntegrations_eSOP-12B"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "eSOP-12B SMT Flat Package with Heatsink Tab, see https://ac-dc.power.com/sites/default/files/product-docs/topswitch-jx_family_datasheet.pdf")
	(tags "Power Integrations K Package")
	(property "Reference" "REF**"
		(at 0 -6.1 0)
		(layer "F.SilkS")
	)
	(property "Value" "PowerIntegrations_eSOP-12B"
		(at 0 6.2 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(clearance 0.2)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd oval
		(at -5.45 -4.45 270)
		(size 0.71 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd oval
		(at -5.45 -2.67 270)
		(size 0.71 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd oval
		(at -5.45 -0.89 270)
		(size 0.71 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd oval
		(at -5.45 0.89 270)
		(size 0.71 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd oval
		(at -5.45 4.45 270)
		(size 0.71 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd oval
		(at 5.45 4.45 270)
		(size 0.71 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd oval
		(at 5.45 2.67 270)
		(size 0.71 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd oval
		(at 5.45 0.89 270)
		(size 0.71 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd oval
		(at 5.45 -0.89 270)
		(size 0.71 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd oval
		(at 5.45 -2.67 270)
		(size 0.71 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd oval
		(at 5.45 -4.45 270)
		(size 0.71 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 0 0 270)
		(size 8.15 5.51)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/PowerIntegrations_eSOP-12B.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
