(footprint "Texas_PWSON-N6"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Plastic Small Outline No-Lead http://www.ti.com/lit/ml/mpds176e/mpds176e.pdf")
	(tags "Plastic Small Outline No-Lead")
	(property "Reference" "REF**"
		(at 0 -2.67 0)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_PWSON-N6"
		(at 0 2.725 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -0.4 -0.65)
		(size 0.6 1)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin_ratio -0.2)
	)
	(pad "" smd roundrect
		(at -0.4 0.65)
		(size 0.6 1)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin_ratio -0.2)
	)
	(pad "" smd roundrect
		(at 0.4 -0.65)
		(size 0.6 1)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin_ratio -0.2)
	)
	(pad "" smd roundrect
		(at 0.4 0.65)
		(size 0.6 1)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin_ratio -0.2)
	)
	(pad "1" smd roundrect
		(at -1.4 -0.95)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -1.4 0)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -1.4 0.95)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at 1.4 0.95)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at 1.4 0)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at 1.4 -0.95)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd rect
		(at 0 0)
		(size 1.5 2.4)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SON.3dshapes/Texas_PWSON-N6.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
