(footprint "PowerMacro_M234_WithHole"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "TO-50-4 Power Macro Package Style M234")
	(tags "TO-50-4 Power Macro Package Style M234")
	(property "Reference" "REF**"
		(at -3.45 -4.5 90)
		(layer "F.SilkS")
	)
	(property "Value" "PowerMacro_M234_WithHole"
		(at 13.75 0 90)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at -3.45 -4.5 90)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -0.7 0 90)
		(size 5.5 5.5)
		(drill 5.5)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" smd rect
		(at -7.5 0 90)
		(size 1.5 7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -0.7 6.8 90)
		(size 7 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 7.5 0 90)
		(size 3.5 10)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -0.7 -6.8 90)
		(size 7 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/PowerMacro_M234_WithHole.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
