(footprint "TO-39-10_Window"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "TO-39-10_Window, Window")
	(tags "TO-39-10_Window Window")
	(property "Reference" "REF**"
		(at 2.92 -5.82 0)
		(layer "F.SilkS")
	)
	(property "Value" "TO-39-10_Window"
		(at 2.92 5.82 0)
		(layer "F.Fab")
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 2.92 -5.82 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole oval
		(at 0 0)
		(size 1.6 1.2)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 0.55767 1.716333)
		(size 1.2 1.2)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 2.01767 2.777085)
		(size 1.2 1.2)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 3.82233 2.777085)
		(size 1.2 1.2)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 5.28233 1.716333)
		(size 1.2 1.2)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 5.84 0)
		(size 1.2 1.2)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 5.28233 -1.716333)
		(size 1.2 1.2)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at 3.82233 -2.777085)
		(size 1.2 1.2)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 2.01767 -2.777085)
		(size 1.2 1.2)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole circle
		(at 0.55767 -1.716333)
		(size 1.2 1.2)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-39-10_Window.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
