(footprint "Potentiometer_Bourns_TC33X_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Potentiometer, Bourns, TC33X, Vertical, https://www.bourns.com/pdfs/TC33.pdf")
	(tags "Potentiometer Bourns TC33X Vertical")
	(property "Reference" "REF**"
		(at 0 -2.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "Potentiometer_Bourns_TC33X_Vertical"
		(at 0 2.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "Wiper may be\nanywhere within\ncircle shown"
		(at -0.15 -0.8 0)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -1.8 -1)
		(size 1.2 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 1.45 0)
		(size 1.5 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -1.8 1)
		(size 1.2 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Potentiometer_SMD.3dshapes/Potentiometer_Bourns_TC33X_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
