(footprint "Potentiometer_Bourns_3339P_Vertical_HandSoldering"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Potentiometer, vertical, Bourns 3339P, hand-soldering, http://www.bourns.com/docs/Product-Datasheets/3339.pdf")
	(tags "Potentiometer vertical Bourns 3339P hand-soldering")
	(property "Reference" "REF**"
		(at 0 -7.6 0)
		(layer "F.SilkS")
	)
	(property "Value" "Potentiometer_Bourns_3339P_Vertical_HandSoldering"
		(at 0 2.52 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at -3.018 -2.54 90)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 1.75 1.75)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at -2.54 -2.54)
		(size 1.75 1.75)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 0 -5.08)
		(size 1.75 1.75)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3339P_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
