(footprint "Potentiometer_Bourns_3386W_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Potentiometer, horizontal, Bourns 3386W, 9.53 x 4.83 x 9.53mm, https://www.bourns.com/docs/Product-Datasheets/3386.pdf")
	(tags "Potentiometer ")
	(property "Reference" "REF**"
		(at 3 -3.3 0)
		(layer "F.SilkS")
	)
	(property "Value" "Potentiometer_Bourns_3386W_Horizontal"
		(at 2.54 3.3 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 2.54 0.195 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole roundrect
		(at 0 0 90)
		(size 1.44 1.44)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.1736111111)
	)
	(pad "2" thru_hole circle
		(at 2.54 0 90)
		(size 1.44 1.44)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 5.08 0 90)
		(size 1.44 1.44)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3386W_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
