(footprint "Potentiometer_Vishay_T93XA_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Potentiometer, horizontal, Vishay, https://www.vishay.com/docs/51026/t93.pdf, 3/8\" x 3/8\" x 3/16\" (9.7 x 9.8 x 5mm max.)")
	(tags "Potentiometer horizontal vishay")
	(property "Reference" "REF**"
		(at 3.4 -3.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "Potentiometer_Vishay_T93XA_Horizontal"
		(at 2.4 3.725 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 2.54 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 1.65 1.65)
		(drill 0.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "2" thru_hole circle
		(at 2.54 0)
		(size 1.65 1.65)
		(drill 0.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 5.08 0)
		(size 1.65 1.65)
		(drill 0.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Vishay_T93XA_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
