(footprint "Skyworks_SKY13575_639LF"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "http://www.skyworksinc.com/uploads/documents/SKY13575_639LF_203270D.pdf")
	(tags "Skyworks")
	(property "Reference" "REF**"
		(at 0 -2.45 0)
		(layer "F.SilkS")
	)
	(property "Value" "Skyworks_SKY13575_639LF"
		(at -0.01 2.01 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 -1.55 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -0.185 0.185)
		(size 0.29 0.29)
		(layers "F.Paste")
	)
	(pad "" smd custom
		(at -0.17 -0.17)
		(size 0.1 0.1)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.13 0.13) (xy -0.16 0.13) (xy -0.16 0.03) (xy 0.04 -0.16) (xy 0.13 -0.16)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "" smd rect
		(at 0.185 -0.185)
		(size 0.29 0.29)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.185 0.185)
		(size 0.29 0.29)
		(layers "F.Paste")
	)
	(pad "1" smd custom
		(at -0.866 -0.601)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.239 0.053) (xy 0.239 0.101) (xy -0.106 0.101) (xy -0.106 -0.099) (xy 0.175 -0.099)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "2" smd rect
		(at -0.772 -0.2)
		(size 0.4 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -0.772 0.2)
		(size 0.4 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd custom
		(at -0.866 0.602)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.239 -0.054) (xy 0.175 0.098) (xy -0.106 0.098) (xy -0.106 -0.102) (xy 0.239 -0.102)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "5" smd custom
		(at -0.4 0.871)
		(size 0.19 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.1 0.101) (xy -0.1 0.101) (xy -0.1 -0.119) (xy -0.025 -0.299) (xy 0.1 -0.299)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "6" smd rect
		(at 0 0.772 90)
		(size 0.4 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd custom
		(at 0.4 0.87)
		(size 0.19 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.1 -0.118) (xy 0.1 0.102) (xy -0.1 0.102) (xy -0.1 -0.298) (xy 0.025 -0.298)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "8" smd custom
		(at 0.871 0.6)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.101 0.1) (xy -0.18 0.1) (xy -0.244 -0.052) (xy -0.244 -0.1) (xy 0.101 -0.1)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "9" smd rect
		(at 0.772 0.2)
		(size 0.4 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 0.772 -0.2)
		(size 0.4 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd custom
		(at 0.872 -0.6)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.1 0.1) (xy -0.245 0.1) (xy -0.245 0.052) (xy -0.181 -0.1) (xy 0.1 -0.1)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "12" smd custom
		(at 0.398 -0.87)
		(size 0.19 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.102 0.118) (xy 0.027 0.298) (xy -0.098 0.298) (xy -0.098 -0.102) (xy 0.102 -0.102)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "13" smd rect
		(at 0 -0.772 90)
		(size 0.4 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd custom
		(at -0.4 -0.869)
		(size 0.19 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.1 0.297) (xy -0.025 0.297) (xy -0.1 0.117) (xy -0.1 -0.103) (xy 0.1 -0.103)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "15" smd custom
		(at 0 0)
		(size 0.29 0.29)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.36 0.36) (xy -0.36 0.36) (xy -0.36 -0.15) (xy -0.14 -0.36) (xy 0.36 -0.36)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF.3dshapes/Skyworks_SKY13575_639LF.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
