(footprint "Skyworks_SKY65404-31"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "http://www.skyworksinc.com/uploads/documents/SKY65404_31_201512K.pdf")
	(tags "Skyworks")
	(property "Reference" "REF**"
		(at 0 -1.75 0)
		(layer "F.SilkS")
	)
	(property "Value" "Skyworks_SKY65404-31"
		(at 0 1.85 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 270)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.725 -0.5)
		(size 0.35 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -0.725 0)
		(size 0.35 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -0.725 0.5)
		(size 0.35 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at 0.725 0.5)
		(size 0.35 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at 0.725 0)
		(size 0.35 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at 0.725 -0.5)
		(size 0.35 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd custom
		(at 0 0)
		(size 0.35 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 0)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.1 -0.6) (xy 0.35 -0.6) (xy 0.35 0.6) (xy 0.1 0.6) (xy 0.1 0.65) (xy -0.1 0.65) (xy -0.1 0.6)
					(xy -0.35 0.6) (xy -0.35 -0.45) (xy -0.2 -0.6) (xy -0.1 -0.6) (xy -0.1 -0.65) (xy 0.1 -0.65)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF.3dshapes/Skyworks_SKY65404-31.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
