(footprint "Pulse_W3011"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Pulse RF Antenna, 4mm Clearance")
	(tags "antenna rf")
	(property "Reference" "REF**"
		(at 0 -3 0)
		(layer "F.SilkS")
	)
	(property "Value" "Pulse_W3011"
		(at 0 3 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "on all layers"
		(at -2.2 0 90)
		(layer "Cmts.User")
	)
	(fp_text user "No copper"
		(at -2.7 0 90)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0.05 -0.05 0)
		(layer "F.Fab")
	)
	(pad "1" smd trapezoid
		(at -0.5 -1.6 90)
		(size 0.8 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd trapezoid
		(at 0 1.6 90)
		(size 0.8 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd trapezoid
		(at 0.5 -1.6 90)
		(size 0.8 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_Antenna.3dshapes/Pulse_W3011.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
