(footprint "Mini-Circuits_HQ1157"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Footprint for Mini-Circuits case HQ1157 (https://www.minicircuits.com/case_style/HQ1157.pdf)")
	(tags "Mini-Circuits HQ1157")
	(property "Reference" "REF**"
		(at 8.128 0 270)
		(layer "F.SilkS")
	)
	(property "Value" "Mini-Circuits_HQ1157"
		(at -8 -0.1 270)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at -0.2 0 270)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at 0 -16.256 270)
		(size 3.048 2.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -3.6195 -9.525 90)
		(size 2.54 3.048)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -3.6195 -5.715 90)
		(size 2.54 3.048)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -3.6195 -1.905 90)
		(size 2.54 3.048)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -3.6195 1.905 90)
		(size 2.54 3.048)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -3.6195 5.715 90)
		(size 2.54 3.048)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -3.6195 9.525 90)
		(size 2.54 3.048)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 0 16.256 270)
		(size 3.048 2.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 3.6195 9.525 270)
		(size 2.54 3.048)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 3.6195 5.715 270)
		(size 2.54 3.048)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 3.6195 1.905 270)
		(size 2.54 3.048)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 3.6195 -1.905 270)
		(size 2.54 3.048)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 3.6195 -5.715 270)
		(size 2.54 3.048)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 3.6195 -9.525 270)
		(size 2.54 3.048)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_Mini-Circuits.3dshapes/Mini-Circuits_HQ1157.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
