(footprint "TD1205"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "https://github.com/Telecom-Design/Documentation_TD_RF_Module/blob/master/TD1205%20Datasheet.pdf")
	(tags "SIGFOX Module")
	(property "Reference" "REF**"
		(at 7 25.5 180)
		(layer "F.SilkS")
	)
	(property "Value" "TD1205"
		(at 13.97 17.78 90)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 11.43 17.78 90)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0 90)
		(size 1.905 1.905)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 26.5 0 90)
		(size 1.905 1.905)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 5.63 23.21 90)
		(size 1.905 1.905)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 8.17 23.21 90)
		(size 1.905 1.905)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 10.71 23.21 90)
		(size 1.905 1.905)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 13.25 23.21 90)
		(size 1.905 1.905)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 15.79 23.21 90)
		(size 1.905 1.905)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at 18.33 23.21 90)
		(size 1.905 1.905)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 20.87 23.21 90)
		(size 1.905 1.905)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_Module.3dshapes/TD1205.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
