(footprint "Relay_DPDT_Hongfa_HF115F-2Z-x4"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Hongfa DPDT power relay, 8A, 250VAC, body size 29x127.x15.7mm, https://source.hongfa.com//pdf/web/viewer.html?file=/Uploads/Product/PDF/HF115F_I_en.pdf")
	(tags "2-Form-C")
	(property "Reference" "REF**"
		(at -0.02 -3.72 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "Relay_DPDT_Hongfa_HF115F-2Z-x4"
		(at 11.9 11.68 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 13.48 10.08 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 13.48 10.08 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 11.9 4.04 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "11" thru_hole circle
		(at 20.16 0)
		(size 2.3 2.3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole circle
		(at 15.12 0)
		(size 2.3 2.3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole circle
		(at 25.2 0)
		(size 2.3 2.3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at 20.16 7.56)
		(size 2.3 2.3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "22" thru_hole circle
		(at 15.12 7.56)
		(size 2.3 2.3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "24" thru_hole circle
		(at 25.2 7.56)
		(size 2.3 2.3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A1" thru_hole roundrect
		(at 0 0)
		(size 2.3 2.3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.1086956522)
	)
	(pad "A2" thru_hole circle
		(at 0 7.56)
		(size 2.3 2.3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_DPDT_Hongfa_HF115F-2Z-x4.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
