(footprint "Relay_SPDT_Finder_36.11"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "FINDER 36.11, SPDT relay, 10A, https://cdn.findernet.com/app/uploads/S36EN.pdf")
	(tags "spdt relay")
	(property "Reference" "REF**"
		(at 6 -4.2 0)
		(layer "F.SilkS")
	)
	(property "Value" "Relay_SPDT_Finder_36.11"
		(at 6 17 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 5.975 6.199999 270)
		(layer "F.Fab")
	)
	(pad "11" thru_hole circle
		(at 6 -2)
		(size 2.4 2.4)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(clearance 0.2)
	)
	(pad "12" thru_hole circle
		(at 12 12.2)
		(size 2.4 2.4)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole circle
		(at 0 12.2)
		(size 2.4 2.4)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A1" thru_hole roundrect
		(at 0 0)
		(size 2.5 2.5)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.1)
	)
	(pad "A2" thru_hole circle
		(at 12 0)
		(size 2.4 2.4)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_SPDT_Finder_36.11.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
