(footprint "R_Shunt_Vishay_WSK2512_6332Metric_T2.66mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Shunt Resistor SMD 2512 (6332 Metric), 2.6mm thick, Vishay WKS2512, Terminal length (T) 2.66mm, 0.5 to 0.99 milli Ohm (http://http://www.vishay.com/docs/30108/wsk.pdf)")
	(tags "resistor shunt WSK2512")
	(property "Reference" "REF**"
		(at 0 -2.65 0)
		(layer "F.SilkS")
	)
	(property "Value" "R_Shunt_Vishay_WSK2512_6332Metric_T2.66mm"
		(at 0 2.65 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -2.48 -0.635)
		(size 3.3 2.03)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.12)
	)
	(pad "2" smd roundrect
		(at -3.43 1.27)
		(size 1.4 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at 3.43 -1.27)
		(size 1.4 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at 2.48 0.635)
		(size 3.3 2.03)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.12)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Shunt_Vishay_WSK2512_6332Metric_T2.66mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
