(footprint "RotaryEncoder_Bourns_Horizontal_PEC09-2xxxF-Sxxxx"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Bourns rotary encoder, PEC09, with switch, horizontal shaft, https://www.bourns.com/products/encoders/contacting-encoders/product/PEC09")
	(tags "rotary encoder")
	(property "Reference" "REF**"
		(at -1.9 -8.7 0)
		(layer "F.SilkS")
	)
	(property "Value" "RotaryEncoder_Bourns_Horizontal_PEC09-2xxxF-Sxxxx"
		(at -1.1 3.9 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 2 -2.5 90)
		(layer "F.Fab")
	)
	(pad "A" thru_hole circle
		(at 0 0)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B" thru_hole circle
		(at 0 -5)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "C" thru_hole circle
		(at 0 -2.5)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "S1" thru_hole circle
		(at -6.25 0)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "S2" thru_hole circle
		(at -6.25 -5)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Rotary_Encoder.3dshapes/RotaryEncoder_Bourns_Horizontal_PEC09-2xxxF-Sxxxx.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
