(footprint "Avago_APDS-9960"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Digital Proximity, Ambient Light, RGB and Gesture Sensor (https://docs.broadcom.com/doc/AV02-4191EN)")
	(tags "DFN Sensor optical IR")
	(property "Reference" "REF**"
		(at 0 -2 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "Avago_APDS-9960"
		(at 0 2.2 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "D"
		(at -0.92 0 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "R"
		(at -1.27 -0.35 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "L"
		(at -1.27 0.35 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "U"
		(at -1.62 0 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "LED"
		(at 1.43 0 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at -0.4 0 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -1.455 -0.7)
		(size 0.72 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -0.485 -0.7)
		(size 0.72 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 0.485 -0.7)
		(size 0.72 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 1.455 -0.7)
		(size 0.72 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 1.455 0.7)
		(size 0.72 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 0.485 0.7)
		(size 0.72 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -0.485 0.7)
		(size 0.72 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -1.455 0.7)
		(size 0.72 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Sensor.3dshapes/Avago_ADPS-9960.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
