(footprint "Sensirion_DFN-4_1.5x1.5mm_P0.8mm_SHT4x_NoCentralPad"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Sensirion, SHT40, SHT41, SHT45, DFN, 4 Pin (https://sensirion.com/media/documents/33FD6951/624C4357/Datasheet_SHT4x.pdf)")
	(tags "DFN NoLead")
	(property "Reference" "REF**"
		(at 0 -1.7 0)
		(layer "F.SilkS")
	)
	(property "Value" "Sensirion_DFN-4_1.5x1.5mm_P0.8mm_SHT4x_NoCentralPad"
		(at 0 1.7 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -0.7 -0.4)
		(size 0.5 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -0.7 0.4)
		(size 0.5 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 0.7 0.4)
		(size 0.5 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 0.7 -0.4)
		(size 0.5 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 0.75 -0.55) (xy 0.45 -0.55) (xy 0.45 -0.25) (xy 0.75 -0.25) (xy 0.75 0.25) (xy 0.45 0.25) (xy 0.45 0.55)
				(xy 0.75 0.55) (xy 0.75 0.75) (xy -0.75 0.75) (xy -0.75 0.55) (xy -0.45 0.55) (xy -0.45 0.25) (xy -0.75 0.25)
				(xy -0.75 -0.25) (xy -0.45 -0.25) (xy -0.45 -0.55) (xy -0.75 -0.55) (xy -0.75 -0.75) (xy 0.75 -0.75)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Sensor_Humidity.3dshapes/Sensirion_DFN-4_1.5x1.5mm_P0.8mm_SHT4x_NoCentralPad.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
