(footprint "TerminalBlock_Degson_DG246-3.81-03P"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "DEGSON ELECTRONICS DG246 terminal block, https://www.degson.com/index.php?a=downloadFile&id=1090277")
	(tags "connector terminal block")
	(property "Reference" "REF**"
		(at 4.9 -3.86 0)
		(layer "F.SilkS")
	)
	(property "Value" "TerminalBlock_Degson_DG246-3.81-03P"
		(at 4.5 10.4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 4.29 3.51 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 2 3)
		(drill 1.15)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole rect
		(at 0 7)
		(size 2 3)
		(drill 1.15)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 3.81 0)
		(size 2 3)
		(drill 1.15)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 3.81 7)
		(size 2 3)
		(drill 1.15)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at 7.62 0)
		(size 2 3)
		(drill 1.15)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at 7.62 7)
		(size 2 3)
		(drill 1.15)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}//TerminalBlock.3dshapes/TerminalBlock_Degson_DG246-3.81-03P.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
