(footprint "TerminalBlock_MaiXu_MX126-5.0-03P_1x03_P5.00mm"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "terminal block MaiXu MX126-5.0-03P, 3 pins, pitch 5mm, size 15.5x7.8mm, drill diameter 1.3mm, pad diameter 2.8mm, https://www.lcsc.com/datasheet/lcsc_datasheet_2309150913_MAX-MX126-5-0-03P-GN01-Cu-S-A_C5188435.pdf, script-generated using https://gitlab.com/kicad/libraries/kicad-footprint-generator/-/tree/master/scripts/TerminalBlock_MaiXu")
	(tags "THT terminal block MaiXu MX126-5.0-03P pitch 5mm size 15.5x7.8mm drill 1.3mm pad 2.8mm")
	(property "Reference" "REF**"
		(at 4.75 -5.12 0)
		(layer "F.SilkS")
	)
	(property "Value" "TerminalBlock_MaiXu_MX126-5.0-03P_1x03_P5.00mm"
		(at 4.75 4.92 0)
		(layer "F.Fab")
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 4.75 2.65 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 2.8 2.8)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.089286)
	)
	(pad "2" thru_hole circle
		(at 5 0)
		(size 2.8 2.8)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 10 0)
		(size 2.8 2.8)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(model "${KICAD9_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_MaiXu_MX126-5.0-03P_1x03_P5.00mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
