(footprint "TerminalBlock_bornier-3_P5.08mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "simple 3-pin terminal block, pitch 5.08mm, revamped version of bornier3")
	(tags "terminal block bornier3")
	(property "Reference" "REF**"
		(at 5.05 -4.65 0)
		(layer "F.SilkS")
	)
	(property "Value" "TerminalBlock_bornier-3_P5.08mm"
		(at 5.08 5.08 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 5.08 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 3 3)
		(drill 1.52)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 5.08 0)
		(size 3 3)
		(drill 1.52)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 10.16 0)
		(size 3 3)
		(drill 1.52)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_bornier-3_P5.08mm.wrl"
		(offset
			(xyz 5.079999924 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
