(footprint "TerminalBlock_4Ucon_1x04_P3.50mm_Vertical"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Terminal Block 4Ucon ItemNo. 10695, vertical (cable from top), 4 pins, pitch 3.5mm, size 15x8.3mm, drill diameter 1.3mm, pad diameter 2.6mm, http://www.4uconnector.com/online/object/4udrawing/10695.pdf, script-generated using https://gitlab.com/kicad/libraries/kicad-footprint-generator/-/tree/master/scripts/TerminalBlock_4Ucon")
	(tags "THT Terminal Block 4Ucon ItemNo. 10695 vertical pitch 3.5mm size 15x8.3mm drill 1.3mm pad 2.6mm")
	(property "Reference" "REF**"
		(at 5.25 -4.82 0)
		(layer "F.SilkS")
	)
	(property "Value" "TerminalBlock_4Ucon_1x04_P3.50mm_Vertical"
		(at 5.25 5.72 0)
		(layer "F.Fab")
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 5.25 3.45 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 2.6 2.6)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.096154)
	)
	(pad "2" thru_hole circle
		(at 3.5 0)
		(size 2.6 2.6)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 7 0)
		(size 2.6 2.6)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 10.5 0)
		(size 2.6 2.6)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(model "${KICAD9_3DMODEL_DIR}/TerminalBlock_4Ucon.3dshapes/TerminalBlock_4Ucon_1x04_P3.50mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
