(footprint "TerminalBlock_CUI_TB007-508-04_1x04_P5.08mm_Horizontal"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Terminal Block CUI TB007-508-04, 4 pins, pitch 5.08mm, size 20.9x10.2mm, drill diameter 1.6mm, pad diameter 2.4mm, https://www.cuidevices.com/product/resource/tb007-508.pdf, script-generated using https://gitlab.com/kicad/libraries/kicad-footprint-generator/scripts/TerminalBlock_CUI")
	(tags "THT Terminal Block CUI TB007-508-04 pitch 5.08mm size 20.9x10.2mm drill 1.6mm pad 2.4mm")
	(property "Reference" "REF**"
		(at 7.92 -6.02 0)
		(layer "F.SilkS")
	)
	(property "Value" "TerminalBlock_CUI_TB007-508-04_1x04_P5.08mm_Horizontal"
		(at 7.92 6.47 0)
		(layer "F.Fab")
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 7.92 0.225 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 2.4 2.4)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.104167)
	)
	(pad "2" thru_hole circle
		(at 5.08 0)
		(size 2.4 2.4)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 10.16 0)
		(size 2.4 2.4)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 15.24 0)
		(size 2.4 2.4)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(model "${KICAD9_3DMODEL_DIR}/TerminalBlock_CUI.3dshapes/TerminalBlock_CUI_TB007-508-04_1x04_P5.08mm_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
