(footprint "TerminalBlock_MetzConnect_360322_1x01_Horizontal_ScrewM3.0_WireProtection"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "single screw terminal block Metz Connect 360322, block size 6x4mm^2, drill diamater 1.5mm, 2 pads, pad diameter 3mm, see http://www.metz-connect.com/de/system/files/METZ_CONNECT_U_Contact_Katalog_Anschlusssysteme_fuer_Leiterplatten_DE_31_07_2017_OFF_024803.pdf?language=en page 133, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_MetzConnect")
	(tags "THT single screw terminal block Metz Connect 360322 size 6x4mm^2 drill 1.5mm pad 3mm")
	(property "Reference" "REF**"
		(at 3 -3.06 0)
		(layer "F.SilkS")
	)
	(property "Value" "TerminalBlock_MetzConnect_360322_1x01_Horizontal_ScrewM3.0_WireProtection"
		(at 3 3.06 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 3 -3.06 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 3 3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 4 0)
		(size 3 3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/TerminalBlock_MetzConnect.3dshapes/TerminalBlock_MetzConnect_360322_1x01_Horizontal_ScrewM3.0_WireProtection.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
