(footprint "TerminalBlock_Philmore_TB132_1x02_P5.00mm_Horizontal"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Terminal Block Philmore , 2 pins, pitch 5mm, size 10x10.2mm, drill diameter 1.2mm, pad diameter 2.4mm, http://www.philmore-datak.com/mc/Page%20197.pdf, script-generated using https://gitlab.com/kicad/libraries/kicad-footprint-generator/-/tree/master/scripts/TerminalBlock_Philmore")
	(tags "THT Terminal Block Philmore  pitch 5mm size 10x10.2mm drill 1.2mm pad 2.4mm")
	(property "Reference" "REF**"
		(at 2.5 -5.92 0)
		(layer "F.SilkS")
	)
	(property "Value" "TerminalBlock_Philmore_TB132_1x02_P5.00mm_Horizontal"
		(at 2.5 6.52 0)
		(layer "F.Fab")
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 2.5 2.8 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 2.4 2.4)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.104167)
	)
	(pad "2" thru_hole circle
		(at 5 0)
		(size 2.4 2.4)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(model "${KICAD9_3DMODEL_DIR}/TerminalBlock_Philmore.3dshapes/TerminalBlock_Philmore_TB132_1x02_P5.00mm_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
