(footprint "TerminalBlock_Phoenix_PTSM-0,5-3-2.5-H-THR_1x03_P2.50mm_Horizontal"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Terminal Block Phoenix PTSM-0,5-3-2.5-H-THR, 3 pins, pitch 2.5mm, size 9.7x10mm, drill diameter 1.2mm, pad diameter 3mm, http://www.produktinfo.conrad.com/datenblaetter/550000-574999/556441-da-01-de-LEITERPLATTENKL__PTSM_0_5__8_2_5_H_THR.pdf, script-generated using https://gitlab.com/kicad/libraries/kicad-footprint-generator/-/tree/master/scripts/TerminalBlock_Phoenix")
	(tags "THT Terminal Block Phoenix PTSM-0,5-3-2.5-H-THR pitch 2.5mm size 9.7x10mm drill 1.2mm pad 3mm")
	(property "Reference" "REF**"
		(at 2.5 -8.32 0)
		(layer "F.SilkS")
	)
	(property "Value" "TerminalBlock_Phoenix_PTSM-0,5-3-2.5-H-THR_1x03_P2.50mm_Horizontal"
		(at 2.5 3.92 0)
		(layer "F.Fab")
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 2.5 -2.2 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 -5)
		(size 1.8 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 1.8 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.138889)
	)
	(pad "2" thru_hole oval
		(at 2.5 -5)
		(size 1.8 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 2.5 0)
		(size 1.8 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at 5 -5)
		(size 1.8 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at 5 0)
		(size 1.8 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(model "${KICAD9_3DMODEL_DIR}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_PTSM-0,5-3-2.5-H-THR_1x03_P2.50mm_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
