(footprint "TerminalBlock_Phoenix_PTSM-0,5-4-HV-2.5-SMD_1x04-1MP_P2.50mm_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "PhoenixContact PTSM0,5 4 HV 2,5mm vertical SMD spring clamp terminal block connector http://www.phoenixcontact.com/us/products/1778719/pdf")
	(tags "2.5mm vertical SMD spring clamp terminal block connector ")
	(property "Reference" "REF**"
		(at -1.4 5.51 0)
		(layer "F.SilkS")
	)
	(property "Value" "TerminalBlock_Phoenix_PTSM-0,5-4-HV-2.5-SMD_1x04-1MP_P2.50mm_Vertical"
		(at 0 -6.3 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 -0.92 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -2.65 1.05)
		(size 1 1)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 2.65 1.05)
		(size 1 1)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" smd rect
		(at -1.25 1.65 180)
		(size 1.2 4.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 1.25 1.65 180)
		(size 1.2 4.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "MP" smd rect
		(at -4.55 -1.05 180)
		(size 2.2 5.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "MP" smd rect
		(at 4.55 -1.05 180)
		(size 2.2 5.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_PTSM-0,5-4-HV-2.5-SMD_1x04-1MP_P2.50mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
