(footprint "TerminalBlock_Phoenix_PTSM-0,5-8-2,5-V-SMD_1x08-1MP_P2.50mm_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "PhoenixContact PTSM0,5 8 2,5mm vertical SMD spring clamp terminal block connector http://www.phoenixcontact.com/us/products/1814760/pdf")
	(tags "PhoenixContact PTSM0.5 8 2.5mm vertical SMD spring clamp terminal block connector ")
	(property "Reference" "REF**"
		(at -1.4 5.53 0)
		(layer "F.SilkS")
	)
	(property "Value" "TerminalBlock_Phoenix_PTSM-0,5-8-2,5-V-SMD_1x08-1MP_P2.50mm_Vertical"
		(at -0.2 -4.88 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 -0.075 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -8.75 2.13 180)
		(size 1.4 3.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -6.25 2.13 180)
		(size 1.4 3.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -3.75 2.13 180)
		(size 1.4 3.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -1.25 2.13 180)
		(size 1.4 3.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 1.25 2.13 180)
		(size 1.4 3.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 3.75 2.13 180)
		(size 1.4 3.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 6.25 2.13 180)
		(size 1.4 3.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 8.75 2.13 180)
		(size 1.4 3.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "MP" smd rect
		(at -12.55 -1.03 180)
		(size 2.3 5.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "MP" smd rect
		(at 12.55 -1.03 180)
		(size 2.3 5.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_PTSM-0,5-8-2,5-V-SMD_1x08-1MP_P2.50mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
