(footprint "TerminalBlock_RND_205-00010_1x11_P5.00mm_Horizontal"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "terminal block RND 205-00010, 11 pins, pitch 5mm, size 55x9mm, drill diameter 1.3mm, pad diameter 2.5mm, http://cdn-reichelt.de/documents/datenblatt/C151/RND_205-00001_DB_EN.pdf, script-generated using https://gitlab.com/kicad/libraries/kicad-footprint-generator/-/tree/master/scripts/TerminalBlock_RND")
	(tags "THT terminal block RND 205-00010 pitch 5mm size 55x9mm drill 1.3mm pad 2.5mm")
	(property "Reference" "REF**"
		(at 25 -6.12 0)
		(layer "F.SilkS")
	)
	(property "Value" "TerminalBlock_RND_205-00010_1x11_P5.00mm_Horizontal"
		(at 25 5.12 0)
		(layer "F.Fab")
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 25 -6.12 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 2.5 2.5)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.1)
	)
	(pad "2" thru_hole circle
		(at 5 0)
		(size 2.5 2.5)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 10 0)
		(size 2.5 2.5)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 15 0)
		(size 2.5 2.5)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 20 0)
		(size 2.5 2.5)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 25 0)
		(size 2.5 2.5)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 30 0)
		(size 2.5 2.5)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at 35 0)
		(size 2.5 2.5)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 40 0)
		(size 2.5 2.5)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole circle
		(at 45 0)
		(size 2.5 2.5)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 50 0)
		(size 2.5 2.5)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(model "${KICAD9_3DMODEL_DIR}/TerminalBlock_RND.3dshapes/TerminalBlock_RND_205-00010_1x11_P5.00mm_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
