(footprint "TerminalBlock_RND_205-00233_1x03_P5.08mm_Horizontal"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "terminal block RND 205-00233, 3 pins, pitch 5.08mm, size 15.2x8.45mm, drill diameter 1.1mm, pad diameter 2.1mm, http://cdn-reichelt.de/documents/datenblatt/C151/RND_205-00232_DB_EN.pdf, script-generated using https://gitlab.com/kicad/libraries/kicad-footprint-generator/-/tree/master/scripts/TerminalBlock_RND")
	(tags "THT terminal block RND 205-00233 pitch 5.08mm size 15.2x8.45mm drill 1.1mm pad 2.1mm")
	(property "Reference" "REF**"
		(at 5.08 -5.52 0)
		(layer "F.SilkS")
	)
	(property "Value" "TerminalBlock_RND_205-00233_1x03_P5.08mm_Horizontal"
		(at 5.08 5.17 0)
		(layer "F.Fab")
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 5.08 -5.52 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 2.1 2.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.119048)
	)
	(pad "2" thru_hole circle
		(at 5.08 0)
		(size 2.1 2.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 10.16 0)
		(size 2.1 2.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(model "${KICAD9_3DMODEL_DIR}/TerminalBlock_RND.3dshapes/TerminalBlock_RND_205-00233_1x03_P5.08mm_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
