(footprint "TerminalBlock_WAGO_233-502_2x02_P2.54mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Terminal Block Wago 233-502, 2 pins, pitch 2.54 mm,  https://www.wago.com/de/leiterplattenanschluss/klemmenleiste-fuer-leiterplatten/p/233-502")
	(tags "THT")
	(property "Reference" "REF**"
		(at -1.27 -3.81 0)
		(layer "F.SilkS")
	)
	(property "Value" "TerminalBlock_WAGO_233-502_2x02_P2.54mm"
		(at 0.64 11.09 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 0.9 2.61 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 1.8 3.2)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.1388888889)
	)
	(pad "1" thru_hole roundrect
		(at 0 5)
		(size 1.8 3.2)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.1388888889)
	)
	(pad "2" thru_hole oval
		(at 2.54 0)
		(size 1.8 3.2)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 2.54 5)
		(size 1.8 3.2)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/TerminalBlock_WAGO.3dshapes/TerminalBlock_WAGO_233-502_2x02_P2.54mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
