(footprint "TerminalBlock_WAGO_804-302_1x02_P7.50mm_45Degree"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Terminal Block WAGO 804-302, 45Degree (cable under 45degree), 2 pins, pitch 7.5mm, size 14x15mm, drill diameter 1.2mm, pad diameter 3mm, , script-generated using https://gitlab.com/kicad/libraries/kicad-footprint-generator/-/tree/master/scripts/TerminalBlock_WAGO")
	(tags "THT Terminal Block WAGO 804-302 45Degree pitch 7.5mm size 14x15mm drill 1.2mm pad 3mm")
	(property "Reference" "REF**"
		(at 4.25 -9.42 0)
		(layer "F.SilkS")
	)
	(property "Value" "TerminalBlock_WAGO_804-302_1x02_P7.50mm_45Degree"
		(at 4.25 7.82 0)
		(layer "F.Fab")
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 4.25 -1.8 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 2 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.125)
	)
	(pad "1" thru_hole rect
		(at 2.5 -5)
		(size 2 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 7.5 0)
		(size 2 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 10 -5)
		(size 2 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(model "${KICAD9_3DMODEL_DIR}/TerminalBlock_WAGO.3dshapes/TerminalBlock_WAGO_804-302_1x02_P7.50mm_45Degree.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
