(footprint "Wuerth_REDCUBE-THR_WP-THRSH_74651175_THR"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "REDCUBE THR with internal through-hole thread WP-THRSH (https://www.we-online.de/katalog/datasheet/74651175.pdf)")
	(tags "screw terminal thread redcube thr power connector")
	(property "Reference" "REF**"
		(at 0 -6 0)
		(layer "F.SilkS")
	)
	(property "Value" "Wuerth_REDCUBE-THR_WP-THRSH_74651175_THR"
		(at 0 6 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd circle
		(at -2.935 -2.935)
		(size 3.1 3.1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at -2.935 2.935)
		(size 3.1 3.1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 2.935 -2.935)
		(size 3.1 3.1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 2.935 2.935)
		(size 3.1 3.1)
		(layers "F.Paste")
	)
	(pad "1" thru_hole circle
		(at -2.935 -2.935)
		(size 3.2 3.2)
		(drill 1.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at -2.935 2.935)
		(size 3.2 3.2)
		(drill 1.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 2.935 -2.935)
		(size 3.2 3.2)
		(drill 1.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 2.935 2.935)
		(size 3.2 3.2)
		(drill 1.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/TerminalBlock_Wuerth.3dshapes/Wuerth_REDCUBE-THR_WP-THRSH_74651175_THR.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
