(footprint "Transformer_NF_ETAL_P3324"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "NF-Transformer, ETAL P3324,http://www.etalgroup.com/sites/default/files/products/P3324_April_2005.pdf")
	(tags "NF-Transformer ETAL P3324 ")
	(property "Reference" "REF**"
		(at -6.35 -6.1 0)
		(layer "F.SilkS")
	)
	(property "Value" "Transformer_NF_ETAL_P3324"
		(at -6.35 13.95 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at -6 11.5 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.52 1.52)
		(drill 0.81)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 0 7.62)
		(size 1.52 1.52)
		(drill 0.81)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at -12.7 7.62)
		(size 1.52 1.52)
		(drill 0.81)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at -12.7 0)
		(size 1.52 1.52)
		(drill 0.81)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Transformer_THT.3dshapes/Transformer_NF_ETAL_P3324.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
