(footprint "Transformer_Toroid_Horizontal_D18.0mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Transformer, Toroid, tapped, horizontal, laying, Diameter 18mm, ")
	(tags "Transformer Toroid tapped horizontal laying Diameter 18mm ")
	(property "Reference" "REF**"
		(at 8.89 -3.81 0)
		(layer "F.SilkS")
	)
	(property "Value" "Transformer_Toroid_Horizontal_D18.0mm"
		(at 8.89 16.51 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 8.89 6.35 0)
		(layer "F.Fab")
	)
	(pad "" thru_hole circle
		(at 8.89 6.35)
		(size 15.24 15.24)
		(drill 8.13)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 2.54 2.54)
		(drill 1.02)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 0 12.7)
		(size 2.54 2.54)
		(drill 1.02)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole rect
		(at 17.78 0)
		(size 2.54 2.54)
		(drill 1.02)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole rect
		(at 17.78 12.7)
		(size 2.54 2.54)
		(drill 1.02)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Transformer_THT.3dshapes/Transformer_Toroid_Horizontal_D18.0mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
