(footprint "Transformer_Wuerth_760871131"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Transformer, horizontal core with bobbin, 14 pin, 2.49 mm pitch, 20 mm row spacing, 25x22.2x16mm https://www.we-online.com/catalog/datasheet/760871131.pdf")
	(tags "transformer flyback")
	(property "Reference" "REF**"
		(at -1 -6 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "Transformer_Wuerth_760871131"
		(at 10 8 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 10 6 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 2 2)
		(drill 1.32)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "2" thru_hole circle
		(at 0 2.49)
		(size 2 2)
		(drill 1.32)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 0 4.98)
		(size 2 2)
		(drill 1.32)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 0 9.98)
		(size 2 2)
		(drill 1.32)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 0 12.47)
		(size 2 2)
		(drill 1.32)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 0 14.96)
		(size 2 2)
		(drill 1.32)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 20 16.195)
		(size 2 2)
		(drill 1.32)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at 20 13.705)
		(size 2 2)
		(drill 1.32)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 20 11.215)
		(size 2 2)
		(drill 1.32)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole circle
		(at 20 8.725)
		(size 2 2)
		(drill 1.32)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 20 6.235)
		(size 2 2)
		(drill 1.32)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole circle
		(at 20 3.745)
		(size 2 2)
		(drill 1.32)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at 20 1.255)
		(size 2 2)
		(drill 1.32)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole circle
		(at 20 -1.235)
		(size 2 2)
		(drill 1.32)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Transformer_THT.3dshapes/Transformer_Wuerth_760871131.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
