(footprint "Valve_ECC-83-1"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Valve ECC-83-1 round pins")
	(tags "Valve ECC-83-1 round pins")
	(property "Reference" "REF**"
		(at -3.45 -16 0)
		(layer "F.SilkS")
	)
	(property "Value" "Valve_ECC-83-1"
		(at -3.45 6.68 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at -3.45 -4.75 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 2.03 2.03)
		(drill 1.02)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 2.15 -2.93)
		(size 2.03 2.03)
		(drill 1.02)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 2.15 -6.58)
		(size 2.03 2.03)
		(drill 1.02)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 0 -9.51)
		(size 2.03 2.03)
		(drill 1.02)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at -3.45 -10.65)
		(size 2.03 2.03)
		(drill 1.02)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at -6.91 -9.51)
		(size 2.03 2.03)
		(drill 1.02)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at -9.06 -6.58)
		(size 2.03 2.03)
		(drill 1.02)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at -9.06 -2.97)
		(size 2.03 2.03)
		(drill 1.02)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at -6.91 0)
		(size 2.03 2.03)
		(drill 1.02)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Valve.3dshapes/Valve_ECC-83-1.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
