(footprint "Valve_Mini_G"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Valve mini G")
	(tags "Valve mini G")
	(property "Reference" "REF**"
		(at -5.08 -2.34 0)
		(layer "F.SilkS")
	)
	(property "Value" "Valve_Mini_G"
		(at 8.38 18.29 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "mounting"
		(at -5.08 8.89 0)
		(layer "Dwgs.User")
	)
	(fp_text user "d=15.6mm"
		(at -5.08 11.18 0)
		(layer "Dwgs.User")
	)
	(fp_text user "${REFERENCE}"
		(at -5.08 2.91 0)
		(layer "F.Fab")
	)
	(pad "" thru_hole circle
		(at -16.51 10.16)
		(size 5 5)
		(drill 4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "" thru_hole circle
		(at 6.35 10.16)
		(size 5 5)
		(drill 4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.78 1.78)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at -10.16 0)
		(size 1.78 1.78)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at -16.51 5.08)
		(size 1.78 1.78)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at -16.51 15.24)
		(size 1.78 1.78)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at -10.16 20.32)
		(size 1.78 1.78)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 0 20.32)
		(size 1.78 1.78)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 6.35 15.24)
		(size 1.78 1.78)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Valve.3dshapes/Valve_Mini_G.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
